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Disclaimer

· We spared no efforts to make sure that the information in this manual is correct and complete. However no liability is accepted for any errors or omissions. Gembird Electronics reserves the right to change the specifications of the hardware and software described in this manual without prior notice.

· No part of this manual may be reproduced, transmitted or translated in any language in any form, by any means, without the prior written permission of Gembird Electronics Ltd.

· Gembird Electronics makes no warranties for damages resulting from corrupted or lost data due to a mistaken operation or malfunction of the product, the software, personal computers or peripheral devices.
Gembird® is a registered trademark of Gembird Europe.

Other names or products not mentioned above may be registered trademarks or trademarks of their respective owners.

Copyright © 1997-2008 Gembird Electronics Ltd. All rights reserved.


Introduction

Thank you for buying our external USB 2.0 enclosure for 2.5 inch HDDs! This manual will help you install it properly. The product is one of the best solutions for mobile storage both for PC and Mac computers.

Features

· Fully compatible with USB 2.0 and USB 1.1 interfaces

· Suitable with all low-profile 2,5" and most of 1.8" hard disk drives

· Hot-swap, Plug-and-Play

· Aluminium case provides the best heat dissipation and hard disk protection

· Cloth or leather pouch
Package contents

· Enclosure

· Windoes98SE driver CD
· USB cable

· Wallet

· mounting screws

· User manual
System requirements

· Personal computer equipped with USB 2.0 port running Windows 98/ME/2000/XP/Vista or Macintosh

· No driver is required with the only exception of Windows 98
Install 2.5” HDD into the enclosure
· Connect the 2.5" hard disk drive to the connector of the enclosure

· Fix the screws tightly
Note

For the new HDD: before installing it into the enclosure, please partition and format the HDD with FAT16 or FAT32 file system. If your HDD format is NTFS or UNIX, please make sure your HDD is reformatted with FAT16 or FAT32 before the connection

Driver installation under Windows 98SE

· Insert the driver CD, and launch "Setup.EXE", the driver will be installed automatically

· Follow the instructions of the installation software until the message "The USB storage driver has been installed completely!" appears.

· Now connect the enclosure (with the HDD inside) with your computer. The system will find the new device automatically and then a [image: image1.png]


 icon will appear in the System tray.
Driver installation under Windows ME/2000/XP/Vista

Under Windows ME/2000/XP/Vista, the system will find and setup the "USB Mass Storage Device" automatically.

Driver installation under Mac OS

If your operating system is Mac OS 8.6 or above the driver will be installed automatically. If you are running an older version of OS you will have to first download and setup "USB MASS STORAGE SUPPORT 1.3.5" from the SOFTWARE SUPPORT website: http://www.apple.com/support 

Congratulation, you can enjoy this product now!
Warning: Before you disconnect the enclosure from your system, you should always perform the following procedure: 

· Click the icon [image: image2.png]


 with your mouse right button 

· Choose "Safely remove hardware" from the popup menu

· After your confirmation the message "Storage device can now be safely removed from the system" will appear.

Only now you can disconnect the enclosure from the computer! 

2.5” external enclosure
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