
;################################################################################ 
;
;
;  Name:	  		RSET8168.100
;
;  Version:	  		V1.00
;
;  Released By:   	Vika Yen
;
;  Release Date:  	10/12/05
;
;  Changed File:    RSET8168.c
;				    PCI.h
;
;  Reason:	  Modify media type and loopback test
;		
;  Comment:       
;            1. Correct media type string, when link status chang
;		     2. Fix IP checksum decision, when IP checksum be 0x0 or 0xFFFF.
		     3. Decrease collision probability in 10M Half, 

;################################################################################ 
;
;
;  Name:	  		RSET8168.101
;
;  Version:	  		V1.01
;
;  Released By:   	Vika Yen
;
;  Release Date:  	02/15/06
;
;  Changed File:    RSET8168.c
;				    
;
;  Reason:	  
;		
;  Comment:       
;            1. Correct the EEPROM content order with RTL8168B
;			 2. Set VPD address start point in 00h
;			 3. Resolve interrupt issue at some platforms
;################################################################################ 
;
;
;  Name:	      	RSET8168.102
;
;  Version:	  	  	V1.02
;
;  Released By:   Vika Yen
;
;  Release Date:  07/05/06
;
;  Changed File:  RSET8168.c
;
;  Reason:	     
;		
;  Comment:       
;	 	          	1. Fix packet issue that cause by CPU speed at loopback mode 
;################################################################################ 
